|  |
| --- |
| **Operating instructions**in keeping with Section 14 of the German Ordinance of Hazardous Substances  |
| **Work area:****Workplace:****Field of activity:** |  |
| **Designation of hazardous substances** |
| **Cleanet® GR 11** |
| **Hazards to man and the environment** |
|  | - |
| **Protective measures and rules of conduct** |
|  | Ensure very good ventilation of the workplace. Do not smoke, eat or drink in work and storage rooms. Also do not store food, drinks or tobacco. Prescribed protective equipment: - Safety goggles or face protection. Report any malfunction immediately to your supervisor. Carry out repairs properly and with caution. Pipelines must be completely drained. Avoid evaporation and splashing during decanting. Only transport fragile containers with the substance using an outer container (e.g. plastic bucket with handle). Only decant into clean and lye resistant containers. |
| **Behaviour in case of danger** |
|  | In the event of fire-fighting, strictly follow operating instructions.Extinguish small fires with CO2 or powder extinguisher and/or with a water spray jet. Dilute with plenty of water if possible. Avoid inhalation of dust, vapours or fumes - use breathing apparatus.If leakage of liquid occurs, inform supervisor or plant management immediately. |
| **First aid** |
|  | Wash affected skin thoroughly with soap and water. In case of extensive skin wetting, rinse immediately with emergency shower and carefullyremove wetted clothing. Then rinse the skin with plenty of water and, if necessary, treat with a detergent such as Diphoterine. After burns, cool skin with cold water until pain disappears. Do not dress face and eye burns. Get medical attention. After eye contact, rinse immediately with water for several minutes and notify supervisor. After occupational care consult an ophthalmologist. After swallowing, drink plenty of water, if available with activated carbon additive. Prevent vomiting if possible. If unconscious, bring into stable side position. Consult a physician. Provide fresh air, rest and warmth after inhalation. Inform a doctor if necessary. |
| **In case of an emergency:** **First responder Attending physician****Emergency call****Fire brigade** |
| **Proper disposal** |
| _Pic29 | Absorb spilled liquid with a suitable universal binder and hand over to the responsible body for disposal, as well as waste in closed containers. Small quantities may be diluted with water and discharged into the sewage system. |
|  **Preparation** **Testing** **Release****Date****Name****Signature** |