|  |
| --- |
| **Operating instructions**in keeping with Section 14 of the German Ordinance of Hazardous Substances |
| **Work area:****Workplace:****Field of activity:** |  |
| **Designation of hazardous substances** |
| **Cleanet® OR 6** |
| **Hazards to man and the environment** |
|  | Harmful to aquatic organisms, with long-term effects. |
| **Protective measures and rules of conduct** |
|  | Ensure very good ventilation of the workplace. Do not smoke, eat or drink in work and storage rooms. Also do not store food, drinks or tobacco. Report any malfunction immediately to your supervisor. Carry out repairs properly and with caution. Pipelines must be completely drained. Only transport fragile containers with the substance using an outer container (e.g. plastic bucket with handle). Only decant into clean and lye resistant containers. |
| **Behaviour in case of danger** |
|  | In the event of fire-fighting, strictly follow operating instructions. |
| **First aid** |
|  | - |
| **In case of an emergency:** **First responder Attending physician****Emergency call****Fire brigade** |
| **Proper disposal** |
| _Pic29 | - |
|  **Preparation** **Testing** **Release****Date****Name****Signature** |